<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="-2.4892" y1="-2.794" x2="-2.7432" y2="-2.54" width="0" layer="20" curve="90"/>
<wire x1="-2.7432" y1="-2.54" x2="-7.493" y2="-2.54" width="0" layer="20"/>
<wire x1="-8.128" y1="-1.905" x2="-11.049" y2="-1.905" width="0" layer="20"/>
<wire x1="-11.049" y1="-1.905" x2="-11.938" y2="-1.016" width="0" layer="20" curve="-90"/>
<wire x1="-11.938" y1="-1.016" x2="-11.938" y2="2.921" width="0" layer="20"/>
<wire x1="-11.938" y1="2.921" x2="-11.049" y2="3.81" width="0" layer="20" curve="-90"/>
<wire x1="-11.049" y1="3.81" x2="2.1082" y2="3.81" width="0" layer="20"/>
<wire x1="2.1082" y1="3.81" x2="2.4892" y2="3.429" width="0" layer="20" curve="-90"/>
<wire x1="2.4892" y1="3.429" x2="2.4892" y2="-2.794" width="0" layer="20"/>
<wire x1="-7.493" y1="-2.54" x2="-8.128" y2="-1.905" width="0" layer="20" curve="90"/>
<text>OSO-MISC-21-016
Power Tester</text>
<text>Must be only power
source to watch.
DO NOT USE ALONG
WITH A COIN CELL!!!</text>
</plain>
<libraries>
<library name="FH19C-9S-0.5SH">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="FH19C9S05SH10-FFC">
<description>&lt;b&gt;FH19C-9S-0.5SH(10)-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B2,54">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REV" value="D"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$3" library="FH19C-9S-0.5SH" package="FH19C9S05SH10-FFC" value="FH19C-9S-0.5SH_10-FFC"/>
<element name="VCC" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="2"/>
<contactref element="GND" pad="TP"/>
</signal>
<signal name="VCC">
<contactref element="U$3" pad="1"/>
<contactref element="VCC" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
